orin

Carrier board DSBOARD-ORNX

jetpack

https://www.forecr.io/blogs/installation/jetpack-5-1-installation-for-dsboard-ornx

Install sdk manager and run it with:

JetPack 5.1 for Target Operating System

Jetson AGX Orin modules for Target Hardware

no Host components

no flash board

Download BSP, extract, update BSP and build rootfs

cd ~/nvidia/nvidia_sdk/JetPack_5.1_Linux_JETSON_AGX_ORIN_TARGETS/Linux_for_Tegra
wget https://github.com/mistelektronik/dsboard_ornx_orin_nx_bsp/raw/master/orin_nx_JP5_1_bsp.tar.xz
tar xf orin_nx_JP5_1_bsp.tar.xz
cp -a orin_nx_JP5_1_bsp/jetson-orin-nx-devkit-16gb.conf orin_nx_JP5_1_bsp/p3768-0000+p3767-0000.conf .
cp orin_nx_JP5_1_bsp/Image kernel/
cp orin_nx_JP5_1_bsp/tegra234-p3767-0000-p3768-0000-a0* kernel/dtb/
cp orin_nx_JP5_1_bsp/tegra234-mb1-bct-gpio-p3767-dp-a03.dtsi bootloader/
cp orin_nx_JP5_1_bsp/tegra234-bpmp-3767-0000-a02-3768-0000-a00.dtb bootloader/t186ref/
cp orin_nx_JP5_1_bsp/tegra234-mb1-bct-p* bootloader/t186ref/BCT/
sudo ./tools/l4t_flash_prerequisites.sh
sudo ./apply_binaries.sh
sudo cp orin_nx_JP5_1_bsp/nvgpu.ko rootfs/usr/lib/modules/5.*/kernel/drivers/gpu/nvgpu/
sed -i "s/cvb_eeprom_read_size = <0x100>;/cvb_eeprom_read_size = <0x0>;/g" bootloader/t186ref/BCT/tegra234-mb2-bct-misc-p3767-0000.dts
sed -i "s/ODMDATA=\"gbe-uphy-config-8,hsstp-lane-map-3,hsio-uphy-config-0\";/ODMDATA=\"gbe-uphy-config-9,hsstp-lane-map-3,hsio-uphy-config-0\";/g" p3767.conf.common

backup

put board in recovery mode

cd ~/nvidia/nvidia_sdk/JetPack_5.1_Linux_JETSON_AGX_ORIN_TARGETS/Linux_for_Tegra
sudo ./tools/backup_restore/l4t_backup_restore.sh -b jetson-orin-nx-devkit-16gb