orin

Carrier board DSBOARD-ORNX

jetpack

https://www.forecr.io/blogs/installation/jetpack-5-1-installation-for-dsboard-ornx

Install sdk manager and run it with:

JetPack 5.1 for Target Operating System

Jetson AGX Orin modules for Target Hardware

no Host components

no flash board

Download BSP, extract, update BSP and build rootfs

cd ~/nvidia/nvidia_sdk/JetPack_5.1_Linux_JETSON_AGX_ORIN_TARGETS/Linux_for_Tegra
wget https://github.com/mistelektronik/dsboard_ornx_orin_nx_bsp/raw/master/orin_nx_JP5_1_bsp.tar.xz
tar xf orin_nx_JP5_1_bsp.tar.xz
cp -a orin_nx_JP5_1_bsp/jetson-orin-nx-devkit-16gb.conf orin_nx_JP5_1_bsp/p3768-0000+p3767-0000.conf .
cp orin_nx_JP5_1_bsp/Image kernel/
cp orin_nx_JP5_1_bsp/tegra234-p3767-0000-p3768-0000-a0* kernel/dtb/
cp orin_nx_JP5_1_bsp/tegra234-mb1-bct-gpio-p3767-dp-a03.dtsi bootloader/
cp orin_nx_JP5_1_bsp/tegra234-bpmp-3767-0000-a02-3768-0000-a00.dtb bootloader/t186ref/
cp orin_nx_JP5_1_bsp/tegra234-mb1-bct-p* bootloader/t186ref/BCT/
sudo ./tools/l4t_flash_prerequisites.sh
sudo ./apply_binaries.sh
sudo cp orin_nx_JP5_1_bsp/nvgpu.ko rootfs/usr/lib/modules/5.*/kernel/drivers/gpu/nvgpu/
sed -i "s/cvb_eeprom_read_size = <0x100>;/cvb_eeprom_read_size = <0x0>;/g" bootloader/t186ref/BCT/tegra234-mb2-bct-misc-p3767-0000.dts
sed -i "s/ODMDATA=\"gbe-uphy-config-8,hsstp-lane-map-3,hsio-uphy-config-0\";/ODMDATA=\"gbe-uphy-config-9,hsstp-lane-map-3,hsio-uphy-config-0\";/g" p3767.conf.common

backup (not working)

disable automount on host

sudo systemctl stop udisks2.service

put board in recovery mode

lsusb | grep 955 Bus 001 Device 007: ID 0955:7323 NVIDIA Corp. APX

backup (output in ./tools/backuprestore/images) <code> cd ~/nvidia/nvidiasdk/JetPack5.1LinuxJETSONAGXORINTARGETS/LinuxforTegra sudo ./tools/backuprestore/l4tbackup_restore.sh -b jetson-orin-nx-devkit-16gb </code>

flash

customize rootfs

sudo tools/l4t_create_default_user.sh -u ubuntu -p ubuntu -a -n orin --accept-license

build image (–no-flash)

sudo ./tools/kernel_flash/l4t_initrd_flash.sh --no-flash --external-device nvme0n1p1 -c tools/kernel_flash/flash_l4t_external.xml -p "-c bootloader/t186ref/cfg/flash_t234_qspi.xml" --showlogs --network usb0 jetson-orin-nx-devkit-16gb internal

put board in recovery mode

flash

sudo ./tools/kernel_flash/l4t_initrd_flash.sh --flash-only --external-device nvme0n1p1 -c tools/kernel_flash/flash_l4t_external.xml -p "-c bootloader/t186ref/cfg/flash_t234_qspi.xml" --showlogs --network usb0 jetson-orin-nx-devkit-16gb internal