Linux

Base

edit /etc/locale.gen and run locale-gen

apt-get install wiringpi python-pip
# test GPIO
gpio readall

camera

pip install "picamera[array]"

raspistill -tl 100 [-t 99999]

See opencv and rasberry