Linux

Base

edit /etc/locale.gen and run locale-gen

apt-get install wiringpi python-pip
# test GPIO
gpio readall

apt install rpi-update rpi-update

camera

pip install "picamera[array]"

raspistill -tl 100 [-t 99999]

picamera

opencv and rasberry

view picamera as normal USB camera

add to /etc/modules

bcm2835-v4l2