gstreamer

debug

mkdir ./tmp
export GST_DEBUG_DUMP_DOT_DIR=./tmp/
# ... run pipeline
cd tmp
dot -Tpng x.xx.xx.xxxxxxxxx-gst-launch.FOO.dot > graph.png

show usb camera

gst-launch-1.0 v4l2src device=/dev/video0 ! xvimagesink

rtsp client

gst-launch-1.0 \
rtspsrc location=rtsp://foscam:foscam1@192.168.2.14:554/videoMain ! rtph264depay \
! h264parse ! avdec_h264 \
! videoconvert ! xvimagesink

hardware decode

F=videos/traffico01-1152x720-1610kb.mkv
gst-launch-1.0 filesrc location=$F ! matroskademux ! queue ! h264parse ! omxh264dec ! autovideoconvert ! xvimagesink

hardware encode

... ! videoconvert ! omxh264enc ! matroskamux ! filesink location=test.mkv