gstreamer

debug

mkdir ./tmp
export GST_DEBUG_DUMP_DOT_DIR=./tmp/
# ... run pipeline
cd tmp
dot -Tpng x.xx.xx.xxxxxxxxx-gst-launch.FOO.dot > graph.png

show usb camera

gst-launch-1.0 v4l2src device=/dev/video0 ! xvimagesink

rtsp client

gst-launch-1.0 \
rtspsrc location=rtsp://foscam:foscam1@192.168.2.14:554/videoMain ! rtph264depay \
! h264parse ! avdec_h264 \
! videoconvert ! xvimagesink

hardware decode

F=videos/traffico01-1152x720-1610kb.mkv
gst-launch-1.0 filesrc location=$F ! matroskademux ! queue ! h264parse ! omxh264dec ! autovideoconvert ! xvimagesink

hardware encode

... ! videoconvert ! omxh264enc ! matroskamux ! filesink location=test.mkv

ocam camera

ffplay -f video4linux2 -s 640x480 -i /dev/video0
Stream #0:0: Video: rawvideo ([186]GR[8] / 0x85247BA), bayer_grbg8, 640x480, 245760 kb/s, 100 fps, 100 tbr, 1000k tbn, 1000k tbc

TODO no

gst-launch-1.0 v4l2src ! 'video/x-bayer,width=1280,height=720,framerate=30/1,format=grbg' ! queue ! fakesink