Radxa Android

Build

Screen resolution

To have full-hd /system/build.prop

video.use.overlay=0

In build system change for example radxaudoocommon/Android.mk and touch file build/tools/buildinfo.sh to rebuild build.prop with “make -j4” operation.

PRODUCT_PROPERTY_OVERRIDES += \ video.use.overlay=0

V4l utils

Decompress v4l-utils into <aosp>/external

Run environment build

Compile

cd v4l-utils-imx_jb4.3_1.1.0-ga/utils/v4l2-ctl mm

Now v4l2-clt is in out/target/product/radxarockpro/system/bin/v4l2-ctl

Upload

./mkimage.sh ota sudo /lab/radxa/upgrade_tool di -b rockdev/Image/boot.img sudo /lab/radxa/upgrade_tool uf rockdev/update.img

Boot animation

Put bootanimation.zip into /system/media folder (see theme repo)

For example

adb remount adb push bootanimation.zip /system/media

Post installation

Screen calibration

TSCalibration2